<html><head><meta name="color-scheme" content="light dark"></head><body><pre style="word-wrap: break-word; white-space: pre-wrap;">%% 
%%  A DANTE-Edition example
%% 
%%  Example 33-03-31 on page 702.
%% 
%%  Copyright (C) 2011 Herbert Voss
%% 
%%  It may be distributed and/or modified under the conditions
%%  of the LaTeX Project Public License, either version 1.3
%%  of this license or (at your option) any later version.
%% 
%%  See http://www.latex-project.org/lppl.txt for details.
%% 
%% 
%% ==== 
% Show page(s) 1
%% 
\documentclass[]{article}
\pagestyle{empty}
\setlength\textwidth{375.57637pt}
\setlength\parindent{0pt}

\usepackage{pst-optexp}

\begin{document}
\begin{pspicture}(11.7,6.4)
  \addtopsstyle{Fiber}{linecolor=red!90!black}\psset{usefiberstyle, optboxwidth=1}
  \pnode(1,6){LD}\pnode([Xnodesep=5.5]LD){CPLin1}\pnode([offset=-2]CPLin1){CPLin2}
  \pnode([Xnodesep=2]CPLin1){CPLout1}\pnode([Xnodesep=2]CPLin2){CPLout2}
  \optbox[endbox, labeloffset=0, fiber]([Xnodesep=0.1]LD)(LD){LD}
  \optmzm([Xnodesep=0.1]LD)([Xnodesep=1.5]LD){MZM}\optamp([Xnodesep=1.5]LD)([Xnodesep=2.5]LD){EDFA}
  \optfilter([Xnodesep=2.5]LD)([Xnodesep=3.5]LD){BPF}\optswitch([Xnodesep=3.5]LD)([Xnodesep=4.5]LD){SW}
  \polcontrol([Xnodesep=4.5]LD)(CPLin1){}
  \optcoupler[labeloffset=-0.4](CPLin1)(CPLin2)(CPLout1)(CPLout2){50\,\%}
  \optamp(CPLout1)([Xnodesep=1]CPLout1){EDFA}\optfilter([Xnodesep=1]CPLout1)([Xnodesep=2]CPLout1){BPF}
  \optbox[endbox, labeloffset=0, conn=f-f]([Xnodesep=2]CPLout1)([Xnodesep=2.2]CPLout1){RX}
  \pnode([Xnodesep=3]CPLout2){LoopRT}\pnode([offset=-3.5]LoopRT){LoopRB}
  \pnode([Xnodesep=-5]CPLin2){LoopLT}\pnode([offset=-3.5]LoopLT){LoopLB}
  \optamp(CPLout2)([Xnodesep=-1]LoopRT){EDFA}
  \psline[linearc=1, style=Fiber]([Xnodesep=-1]LoopRT)(LoopRT)([offset=-2]LoopRT)
  \psline[linearc=1, style=Fiber]([offset=1.5]LoopRB)(LoopRB)([Xnodesep=-1]LoopRB)
  \optfiber[labelalign=b, labeloffset=-1]([Xnodesep=-3]LoopRB)([Xnodesep=-1]LoopRB){%
    \begin{tabular}{c}conventional\\fibre 89.8~km\end{tabular}}
  \optamp([Xnodesep=-3]LoopRB)([Xnodesep=-4.5]LoopRB){EDFA}
  \optfilter([Xnodesep=-4.5]LoopRB)([Xnodesep=-6]LoopRB){BPF}
  \optfiber[fiberloops=1, labeloffset=-1, labelalign=b]([Xnodesep=-8.5]LoopRB)([Xnodesep=-6]LoopRB){DCF 16.2~km}
  \optamp([Xnodesep=-8.5]LoopRB)(LoopLB){EDFA}
  \psline[style=Fiber,linearc=1](LoopLB)([Xnodesep=-1]LoopLB)([Xnodesep=-1, offset=3.5]LoopLB)(LoopLT)
  \optfilter(LoopLT)([Xnodesep=1.5]LoopLT){BPF}
  \optswitch([Xnodesep=1.5]LoopLT)([Xnodesep=3.5]LoopLT){SW}
  \polcontrol([Xnodesep=3.5]LoopLT)(CPLin2){}
\end{pspicture}
\end{document}
</pre></body></html>